1. Select the device from device manager. In your case, please select CY7C68001.

A screenshot of a social media post

Description automatically generated

1. Right on the device and choose the “Update driver” option.

A screenshot of a cell phone

Description automatically generated

1. Select “Browse my computer for driver software” option.

A screenshot of a cell phone

Description automatically generated

1. Next, select “Let me pick from a list of available drivers on my computer” option.

A screenshot of a social media post

Description automatically generated

1. Click on “Show All Devices” and then “Next”.

A screenshot of a cell phone

Description automatically generated

1. Now select “Have Disk”.

A screenshot of a cell phone

Description automatically generated

1. In the popup window, click on “Browse”.

A screenshot of a cell phone

Description automatically generated

1. Navigate to the folder where you have saved the driver folder. Go to the appropriate OS version folder and then architecture folder for your host PC. Once the \*.inf file is seen in that path as shown below, click on “Open”.

A screenshot of a cell phone

Description automatically generated

1. Ensure that the correct path appears in the box as per your selection in step 8 and click “OK”.

A screenshot of a cell phone

Description automatically generated

1. Select a suitable model from the list that the device will enumerate with. If SX2 is not present on the list, select any other suitable name. Once the binding is complete, the device will be visible with that name in the device manager. Click “Next”.

A screenshot of a cell phone

Description automatically generated

1. Click “Yes” if the warning appears on your PC.

A screenshot of a cell phone

Description automatically generated

1. If the driver binding is completed successfully, the below message will appear and the device should be present without any yellow mark in the device manager.

A screenshot of a cell phone

Description automatically generated